# FLEXmount DFM200 ADHESIVE

**Temp Range: -40ºC - +150 ºC**

**Min. Application Temp: +10ºC**

**Face:**

White polyester film coated on both sides with high tack permanent pressure sensitive acrylic adhesive and backed on one side with smooth clear polyester release liner and on the other side with a lay-flat release liner.

**Thickness: 35-38micron ±10%**

