**Face:**

Textured polycarbonate film. High temperature resistance and excellent dimensional stability. Ideal for screen printing, automotive, overlays, membrane switches etc.

**Thickness: 250 micron ±5%**

# VELVET/MATTE POLYCARBONATE 250mic

A screenshot of a computer

Description automatically generated