**Face:**

Opaque, rigid PVC film, impact modified

**Thickness: 600micron ±10%**

# MARK RESIST PVC

A screenshot of a computer

Description automatically generated