# 4 YEAR POLYMERIC HI-TACK VINYL

**Temp Range: -30ºC - +100ºC**

**Min. Application Temp: +5ºC**

**Face:**

A high tack adhesive to solve the problem of adhesion onto smooth low energy surfaces including Polypropylene, Polyethylene and ABS. Suitable for durable graphics on extreme sports equipment. The 100-micron film is easy for printing, cutting and application. Resistant to oils, fats, fuels, solvents, mild acids and alkali.

**Thickness: 100 micron ±5%**

**Adhesive:**

High-tack permanent, solvent-based acrylic adhesive.

**Liner**

Layflat kraft paper with PE coating.

**Basic Weight: 140 gsm**